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® Suitable for global usage in modem and fax
applications

® Surface-mount package, supplied in tape & reel
® PCMCIA-Il in-card version available

® UL 60950 Recognized (file E216510) “

(supplementary insulation, 250VAC
working voltage)
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